The IS AC/DC relay is a very versatile relay as it will operate on AC voltages ranging from 8 volts to 32 volts, and it will also operate on DC voltages ranging from 10 volts to 35 volts.

**(IS AC/DC)**

**AC/DC RELAY**

The double pole relay is a simple to fit module wherever a dry contact, voltage free switching is required or where there is a need for higher than usual currents and voltages to be switched. The double pole relay is rated at 8 Amps complete with LED indication.

* Works on AC or DC
* Automatic voltage selection
* No jumper links to select voltage
* Not polarity conscious.
* Energy saving feature that allows the relay to work at higher voltages

|  |  |
| --- | --- |
| Supply Voltage | 6 - 32 Volts AC  10 – 35 Volts AC |
| Coil Resistance | 360 Ohms |
| Nominal Current | 20 mA |
| Double Pole Relay rated at | 8 Amps at 240 V AC  8 Amps at 30 V DC |
| Minimum switching current | 10 mA (to keep contacts clean) |
| Dimensions | 56mm (W)  69mm (L)  30mm (H) |

We recommend IS Sticky Feet Size B,

self-adhesive mounting pillars to ensure

a neat fixing.



