This is the miniature version of the IS 12.

**(IS M12)**

**12 VOLT MINI POLARISED RELAY**

The 12 volt polarised double pole relay is a simple to fit module wherever a dry contact, voltage free switching is required. It is ideal for low current low voltage switching i.e. CCTV systems, industrial control systems and many other applications. The double pole relay is rated at 2 Amps complete with LED indication. It is supplied as an individual unit or in a strip of 4 modules.

|  |  |
| --- | --- |
| Supply Voltage | 12 Volts DC |
| Coil Resistance | 285 Ohms |
| Nominal Current | 60 mA |
| Double Pole Relay rated at | 2 Amps at 30 V DC minimum 10 mA |
| Dimensions | Single:  37m (W)  37mm (L)  16mm (H)  Strip of 4:  37m (W)  150mm (L)  16mm (H) |
| Packing Weight | Single: 30g  Strips of 4: 68g |

We recommend IS Sticky Feet Size A,

self-adhesive mounting pillars to ensure

a neat fixing.



