This is the transistorised miniature version of the IS 24. It is a double pole relay complete

**(IS M24T)**

**24 VOLT MINI TRANSISTORISED RELAY**

with LED indication. It has been designed to allow low current, low voltage signalling outputs from control equipment to activate the relay without overloading the signalling circuits. The trigger voltage may be negative or positive and between 5 and 24 Volts with an approximate current drain of 4 mAmps. The trigger polarity is selected by a plug in link.

It is supplied as an individual unit or in strips of 4 modules.

|  |  |
| --- | --- |
| Supply Voltage | 24 Volts DC |
| Trigger Voltage | 5V – 24V |
| Trigger Current | 4 mA |
| Nominal Current | 30 mA |
| Coil Resistance | 1100 Ohms |
| Double Pole Relay rate at | 2 Amps at 30 V DC |
| Dimensions | Single:37m (W)37mm (L)16mm (H)Strip of 4:37m (W)150mm (L)16mm (H) |
| Packing Weight | Single: 24gPack of 4: 74g |

We recommend IS Sticky Feet Size A,

self-adhesive mounting pillars to ensure

a neat fixing.



