This is the miniature version of the IS 24. The 24 volt polarised double pole relay is a simple

**(IS M24)**

**24 VOLT MINI POLARISED RELAY**

to fit module wherever a dry contact, voltage free switching is required. It is ideal for low

current low voltage switching i.e. Industrial control systems and many other applications. The double pole relay is rated at 2 Amps complete with LED indication. It is supplied as an individual unit or in a strip of 4 modules.

|  |  |
| --- | --- |
| Supply Voltage | 12 Volts DC |
| Coil Resistance | 1100 Ohms |
| Nominal Current | 60 mA |
| Double Pole Relay rate at | 2 Amps at 30 V DC |
| Dimensions | Single:37m (W)37mm (L)16mm (H)Strip of 4:37m (W)150mm (L)16mm (H) |
| Packing Weight | Single: 22gStrip of 4: 72g |

We recommend IS Sticky Feet Size A,

self-adhesive mounting pillars to ensure

a neat fixing.



